17.2, 19.2, & 26.2 Stippled Grip by Chairmanwon

https://odysee.com/@chairmanwon:a/FMDA-DD26.2-CHAIRMANWON-STIPPLE-PACK:a

No funtional or geometric changes outside of the grips. The process I use to apply the stipple is mesh based so there is no way to include a STEP file.

Versions with the AVES logo in the grip can be found at my website https://origamifaceshield.com/ but are not included in the FMDA release.

The only changes that you need to make vs the normal FMDA profile are as follows

Support X/Y Distance: 1.1mm (stops Cura from supporting stipples)
Use tree supports instead of normal supports

I have tested this frame using ESUN PLA+ using the settings in the FMDA README file which I have pasted below in case this zip gets shared on its own.

Nozzle: 0.4mm
Layer Height: 0.15mm
Temp: 230/60C
Infill: 100% (You can use 99% infill on Cura to speed up the print time)
Supports: On/full - use a close support interface gap. Your interface gap should not be larger than 0.15mm unless you know what you are doing with your setup.
Cooling fan: 20% normal, 50% on bridges. Off for the first 10 layers. Keep the fan low to prevent warp.

Post processing: If you print your frame upright, you can clean up the rough bottom-facing areas of your print with a soldering iron - after removing supports, take your soldering iron and melt the rough patches on the frame together to make them smooth.

All other settings can/should be left as default or whatever you know works best with your printing setup.